<Add vessel="reactor" reagent="Sodium methoxide" volume="all" aspiration_speed="[2.0]" prime_n_times="0" priming_volume="0" />
<Add vessel="Sodium methoxide" reagent="[methanol]" volume="5 mL" prime_n_times="0" priming_volume="0" />
<Add vessel="Sodium methoxide" reagent="argon" volume="20 mL" speed="[100.0]" move_speed="100.0" aspiration_speed="[50.0]" prime_n_times="0" priming_volume="0" />
<Add vessel="reactor" reagent="Sodium methoxide" volume="all" prime_n_times="0" priming_volume="0" />
<Add vessel="reactor" reagent="[dimethyl malonate]" volume="2.321 mL" stir="True" aspiration_speed="2.0" />
<HeatChill vessel="reactor" temp="[25 °C]" time="[60 min]" stir="True" />
<HeatChillToTemp vessel="reactor" temp="[3 °C]" stir="True" />
<Add vessel="reactor" reagent="Prenyl bromide" volume="10 mL" time="20 min" stir="[True]" prime_n_times="0" priming_volume="0" />
<Add vessel="Prenyl bromide" reagent="methanol" volume="3 mL" prime_n_times="0" priming_volume="0" />
<Add vessel="Prenyl bromide" reagent="argon" volume="10 mL" speed="50.0" move_speed="50.0" aspiration_speed="50.0" prime_n_times="0" priming_volume="0" />
<Add vessel="reactor" reagent="Prenyl bromide" volume="all" stir="True" prime_n_times="0" priming_volume="0" />
<HeatChill vessel="reactor" temp="[5 °C]" time="4 h" stir="True" />
<Evaporate vessel="reactor" temp="[50 °C]" pressure="[50 mbar]" mode="auto" />
<Add vessel="reactor" reagent="diethyl ether" volume="22 mL" stir="True" prime_n_times="0" />
<Stir vessel="reactor" time="5 min" />
<Transfer from_vessel="reactor" to_vessel="separator" volume="all" />
<Add vessel="separator" reagent="water" volume="5 mL" />
<Separate purpose="[wash]" from_vessel="separator" separation_vessel="separator" to_vessel="[rotavap]" product_phase="top" solvent="aq NaHCO3-brine" through="MgSO4" solvent_volume="40 mL" waste_phase_to_vessel="separator" />
<Separate purpose="[extract]" from_vessel="separator" separation_vessel="separator" to_vessel="rotavap" product_phase="top" solvent="diethyl ether" through="MgSO4" repeats="3" />
<Transfer from_vessel="Et2O" to_vessel="[rotavap]" volume="20 mL" through="MgSO4" move_speed="10.0" />
<Transfer from_vessel="flask_argon_bb" to_vessel="rotavap" volume="50 mL" through="MgSO4" move_speed="50.0" />
<Evaporate vessel="rotavap" temp="50 °C" pressure="218 mbar" time="[30 min]" mode="auto" />
<Dry vessel="rotavap" time="[10 min]" temp="[50 °C]" />