Write UCLID5 code to complete the following task.

> Let C1 be a circuit without input variables and with output variable y1 and register r1. The control function for the output variable transition is y1'=r1, i.e., on the next step y1 is equal to the value of r1 from the previous step. The control function for the register variable transition is r1' = !r1. Circuit C2 has input variable x2, output variable y2, and register variable r2 with the control functions: y2'= x2' OR r2 r2'=x2' OR r2 Model the synchronous composition of these two circuits. Use the variable names y1, r1, x2, y2, and r2.

Reply with your UCLID5 code inside one unique code block.

I can definitely do that! Here is the UCLID5 code:
```
