[Prefered_adjusted_acute_angles_in_PCs.fig] is the figure that contains the contents in below:

**Table 1: Probability distribution of preferred adjusted acute angles in pinwheel centers.** 

| Adjusted acute angle range (degrees) | Probability (%) |
|-------------------|-----------------|
| 0 - 9                   | 0                       |
| 9 - 18                 | 0                       |
| 18 - 27               | 1.30                 |
| 27 - 36               | 0                       |
| 36 - 45               | 3.90                 |
| 45 - 54               | 6.49                 |
| 54 - 63               | 5.19                 |
| 63 - 72               | 14.29               |
| 72 - 81               | 22.08               |
| 81 - 90               | 46.75               |

**Table 1** indicates that PCs are more frequently associated with larger acute angles (closer to orthogonal, 90°), reflecting PC's preference for orthogonal junctions.

Thank you for your thoughtful feedback and for taking the time to review our work. 
